Intermediate Clutch Assembly Removal. Chevrolet Export Express 2000

For 1990-2009 cars

1. Remove the intermediate clutch backing plate retainer ring (629).
2. Remove the intermediate clutch backing plate (630) and the intermediate clutch plates (631, 632) (4 each).
3. Remove the intermediate clutch wave plate (684).
4. Inspect the intermediate clutch plates (631, 632, 684) for the following conditions:

• | Wear

• | Pitting

• | Flaking

• | Cracks

5. Inspect the intermediate clutch backing plate (630) for the following conditions:

• | Burrs

• | Dirt