Overrun Clutch Assembly Disassemble. Chevrolet Export Chevy P42 Commercial Chassis 1999

For 1990-2009 cars

#### Tools Required

• | J 38734 Intermediate Spring Compressor Adapter

• | J 23327 Clutch Spring Compressor

1. Separate the overdrive carrier assembly (514) from the overrun clutch housing assembly (504).
2. Remove the overrun clutch backing plate retainer ring (511) from the overrun clutch housing assembly (504).
3. Remove the overrun clutch backing plate (510) and the overrun clutch plates (508, 509) (3 steel and 3 composite).
4. Inspect the overrun clutch plates (508-510) for burning, scoring, flaking, pitting, and wear.
5. Using the J 23327 and the J 38734 , remove the overrun clutch spring assembly (506).
6. Remove the overrun clutch spring retainer ring (507).
7. Remove the tools.
8. Remove the overrun clutch spring assembly (506).
9. Remove the overrun clutch piston assembly (505).
10. Inspect the overrun clutch spring assembly (506) for collapsed coils and distortion.
11. Inspect the overrun clutch piston assembly (505) for cracks and a cut seal.
12. Inspect the overrun clutch housing assembly (504) for wear, clogged lubrication holes, and damaged thrust surfaces.