Low and Reverse Band Servo Piston Pin Check. Chevrolet Export Express 2000

For 1990-2009 cars

#### Tools Required

• | J 21370-10 Band Apply Pin Gauge

• | J 38737 Band Apply Pin Checking Tool

1. Install the J 21370-10 into the low and reverse band servo pin bore.
2. Position the J 38737 over the low and reverse band servo bore with the hex hub facing the parking pawl linkage.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Fasten the J 38737 to the case with 2 low and reverse band servo cover bolts (61).

Tighten
Tighten the bolts to 24 N·m (18 lb ft).

4. Verify that the J 21370-10 moves freely in the J 38737 and in the low and reverse band servo pin bore.

Important: The hex hub of the J 38737 must be tightened in order to determine the correct low and reverse band servo piston pin length.

5. Tighten the hex hub of the J 38737 .

Tighten
Tighten the hex hub of the J 38737 to 34 N·m (25 lb ft).

6. Observe the lands on the J 21370-10 in order to determine which land is even with the top edge of the J 38737 . Note the letter (A, B or C) stamped on the J 21370-10 .
7. Refer to the Low and Reverse Band Servo Piston Pin Specification chart, in the Transmission General Specifications , in order to determine the correct pin length to use.
8. Remove the tools.