Intermediate Clutch Piston Travel Check. Chevrolet Export Chevy P32 RV/VAN Chassis 1999

For 1990-2009 cars

1. Using a feeler gage, measure the piston travel between the intermediate clutch backing plate and the intermediate clutch backing plate retaining ring (629).

Piston Travel Specification
Piston travel should be 1.02-2.72 mm (0.040-0.107 in).

2. If piston travel is not correct, inspect for the following conditions and repair as required.

• | Proper assembly

• | Dirt or burrs

• | Worn clutch plates, backing plate, or wave plate

• | Worn case area in the snap ring groove