US English/Metric Conversion. Chevrolet Export Chevy P32 RV/VAN Chassis 1999

For 1990-2009 cars

In order to convert English units to metric units, multiply the English units by the conversion factor shown in the conversion table.

In order to convert metric units to English units, divide the metric units by the conversion factor shown in the conversion table.

English | Multiply/ Divide by | Metric
--- | --- | ---
LENGTH
in | 25.4 | mm
ft | 0.3048 | m
yd | 0.9144
mi | 1.609 | km
AREA
sq in | 645.2 | sq mm
6.45 | sq cm
sq ft | 0.0929 | sq m
sq yd | 0.8361
VOLUME
cu in | 16,387.0 | cu mm
16.397 | cu cm
0.0164 | L
qt | 0.9464
gal | 3.7854
cu yd | 0.7646 | cu m
MASS
lb | 0.4536 | kg
ton | 907.18
0.907 | tonne (t)
FORCE
kg | 9.807 | newtons (N)
oz | 0.2780
lb | 4.448
ACCELERATION
ft/s² | 0.3048 | m/s²
in/s² | 0.0254
TORQUE
lb in | 0.11298 | N·m
lb ft | 1.3558
POWER
hp | 0.746 | kW
PRESSURE (STRESS)
inches of Mercury | 3.377 | kPa
inches of H2O | 0.2491 | kPa
lb/sq in | 6.895
LIGHT
Foot Candle | 10.764 | lm/m²
VELOCITY
mph | 1.6093 | km/h
TEMPERATURE
°F | 5/9(°F-32) | °C
°C | 9/5(°C+32) | °F
FUEL PERFORMANCE
mpg | 2.3527 | L/km