Turbine Shaft Assemble. Chevrolet Export Chevy P32 RV/VAN Chassis 1999

For 1990-2009 cars

#### Tools Required

• | J 38736-1 Turbine Shaft Seal Installer

• | J 38736-2 Turbine Shaft Seal Installer

• | J 38736-3 Turbine Shaft Seal Sizer

• | J 38736-4 Turbine Shaft Seal Sizer

• | J 38736-5 Turbine Shaft Seal Pusher

• | J 38736-6 Turbine Shaft Seal Pusher

1. Place the J 38736-1 onto the turbine shaft (502).
2. Set the J 38736-1 to position #1.
3. Using the J 38736-5 , install the lower turbine shaft intermediate oil seal ring (501).
4. Remove the tools.

Important: Be sure to use the small chamfered end of the J 38736-3 in order to size the lower turbine shaft intermediate oil seal ring. Then use the larger chamfered end of the J 38736-3 in order to size the upper turbine shaft intermediate oil seal ring.

5. With the small chamfered end down, place the J 38736-3 over the lower turbine shaft intermediate oil seal ring.
6. Leave the J 38736-3 on the turbine shaft intermediate oil seal ring for at least 1 minute in order to allow the seal ring to become the proper size.
7. Place the J 38736-1 onto the turbine shaft (502).
8. Set the J 38736-1 to position #2.
9. Using the J 38736-5 , install the upper turbine shaft intermediate oil seal ring (501).
10. Remove the tools.
11. With the large chamfered end down, place the J 38736-3 over the turbine shaft intermediate oil seal ring.
12. Leave the J 38736-3 on the turbine shaft intermediate oil seal ring for at least 1 minute to allow the seal ring to become the proper size.
13. Turn the turbine shaft (502) over.
14. Place the J 38736-2 onto the turbine shaft.
15. Set the J 38736-2 to position #1.
16. Using the J 38736-6 , install the lower turbine shaft rear oil seal ring (503).
17. Remove the tools.

Important: Be sure to use the small chamfered end of the J 38736-4 in order to size the lower turbine shaft rear oil seal ring. Then use the larger chamfered end of the J 38736-4 in order to size the upper turbine shaft rear oil seal ring.

18. With the small chamfered end down, place the J 38736-4 over the lower turbine shaft rear oil seal ring.
19. Leave the J 38736-4 on the turbine shaft rear oil seal ring for at least 1 minute in order to allow the seal ring to become the proper size.
20. Place the J 38736-2 onto the turbine shaft (502).
21. Set the J 38736-2 to position #2.
22. Using the J 38736-6 , install the upper turbine shaft rear oil seal ring (503).
23. Remove the tools.
24. With the large chamfered end down, place the J 38736-4 over the turbine shaft rear oil seal ring.
25. Leave the J 38736-4 on the turbine shaft rear oil seal ring for at least 1 minute in order to allow the seal ring to become the proper size.