Input Shaft Bearing Retainer Assembly. Chevrolet Export Chevy P42 Commercial Chassis 1999

For 1990-2009 cars

### Removal Procedure

Remove the seal from the main drive gear bearing retainer. Pry the seal out with a small pry bar or the equivalent.

### Installation Procedure

#### Tools Required

J 38807 Main Drive Gear Bearing Retainer Seal Installer

Install the oil seal into the main drive gear bearing retainer. The lip of the seal goes toward the installing tool. Use the J 38807 .