Fastener Tightening Specifications. Chevrolet Export Express 2000

For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Size | Spefication
--- | --- | --- | --- | ---
Metric | English
Accumulator Cover to Case | 58 | 1 | M6x1.0x65 | 8-14 N·m | 6-10 lb ft
Accumulator Cover to Case | 59 | 2 | M6x1.0x35 | 8-14 N·m | 6-10 lb ft
A/Trans Case Extension (Y-Car) | 100 | 1 | M10x1.5x55 | 18-22 N·m | 13-16 lb ft
Converter Housing to Case | 94 | 8 | M10x1.5gx45 | 65-75 N·m | 48-55 lb ft
Cooler Pipe Connector | 95 | 2 | 1/4-18NSPS(SPL) | 35-41 N·m | 26-30 lb ft
Detent Spring to Valve Body | 64 | 1 | M8x1.25x20 | 20-27 N·m | 15-20 lb ft
Extension Housing to Case | 32 | 6 | M10x1.5x33.4 | 42-48 N·m | 31-35 lb ft
Extension Housing to Case (4WD Shipping) | N/A | 4 | M10x1.5x33.4 | 11-23 N·m | 8-17 lb in
Forward Accumulator Cover to Valve Body | 364 | 3 | M6x1.0x17.7 | 8-14 N·m | 6-10 lb ft
Line Pressure Test Hole Plug | 39 | 1 | 1/8-27NPTF | 8-14 N·m | 6-10 lb ft
Manual Shaft to Detent Lever Nut | 90 | 1 | M10x1.5 | 27-34 N·m | 20-25 lb ft
Oil Cooler Pipe Fitting | 10 | 2 | 1/4-18NPS(SPL) | 35-41 N·m | 26-30 lb ft
Oil Pan to Case | 76 | 17 | M8x1.25x19.3 | 10-14 N·m | 7-10 lb ft
Oil Passage Cover (Spacer Plate Support) to Case | 77 | 3 | M6x1.0x17.7 | 8-14 N·m | 6-10 lb ft
Park Lock Bracket to Case | 87 | 1 | M8x1.25x20 | 27-34 N·m | 20-25 lb ft
Plate to Case (Shipping) | N/A | 2 | M10x1.5x35 | 27-34 N·m | 20-25 lb ft
Plate to Converter (Shipping) | N/A | 1 | M10x1.5x25 | 27-34 N·m | 20-25 lb ft
Plate to Converter (Shipping) | N/A | 1 | M10x1.5x15 | 27-34 N·m | 20-25 lb ft
Plug Assembly, Oil Pan (C/K) | 107 | 1 | M12x1.75x19.25 | 30-40 N·m | 22-30 lb ft
Plug Assembly, Oil Pan (Y-car) | 101 | 1 | M16x1.50x16 | 28-32 N·m | 21-24 lb ft
Pressure Control Solenoid Bracket to Valve Body Bolt | 364 | 1 | M6x1.0x17.7 | 8-14 N·m | 6-10 lb ft
Pump Assembly to Case | 2 | 7 | M8x1.25x60 | 26-32 N·m | 19-24 lb ft
Pump Cover to Pump Body | 233 | 5 | M8x1.25x40 | 20-27 N·m | 15-20 lb ft
Speed Sensor to Case | 35 | 1 | M6x1.0x15 | 11-14 N·m | 8-10 lb ft
TCC Solenoid Assembly to Case | 68 | 2 | M6x1.0x12 | 8-14 N·m | 6-10 lb ft
Transmission Fluid Pressure (TFP) Manual Valve Position Switch to Body | 70 | 2 | M6x1.0x17.7 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | 62,58 | 3 | M6x1.0x65 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | N/A | 3 | M6x1.0x54.4 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | N/A | 9 | M6x1.0x47.5 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | 59 | 4 | M6x1.0x35 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | 64 | 3 | M8x1.25x20 | 8-14 N·m | 6-10 lb ft
Valve body to Case | 68 | 2 | M6x1.0x12 | 8-14 N·m | 6-10 lb ft
Valve Body to Case | 70,77 | 7 | M6x1.0x18 | 8-14 N·m | 6-10 lb ft
* Reference Number refers to the callout number on the disassembled view.