Fastener Tightening Specifications. Chevrolet Export Chevy P42 Commercial Chassis 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 27 N·m | 20 lb ft
Countershaft Rear Retainer Bolts | 35 N·m | 26 lb ft
Fill Plug | 41 N·m | 30 lb ft
Input Shaft Retainer Bolts | 31 N·m | 23 lb ft
Mainshaft Bearing Retainer Bolts | 35 N·m | 26 lb ft
Mainshaft Nut (RWD models) | 441 N·m | 325 lb ft
Mainshaft Nut (4WD models) | 540 N·m | 400 lb ft
Power Take-off (PTO) Cover Bolts | 41 N·m | 30 lb ft
Shift Cover Bolts | 27 N·m | 20 lb ft
Shift Tower Bolts | 11 N·m | 97 lb in
Speed Sensor Bolt | 22 N·m | 16 lb ft
Transmission Extension Bolts | 54 N·m | 40 lb ft