SMU - SEC. 8A - FUEL GAUGE LEV. - REV. DIAG.. Chevrolet Export Chevy P32 RV/VAN Chassis 1998

For 1990-2009 cars

# SMU - SEC. 8A - FUEL GAUGE LEV. - REV. DIAG.

#### SUBJECT: SMU - SECTION 8A - FUEL GAUGE LEVEL- REVISED DIAGNOSTIC "FUEL GAUGE INACCURATE"

#### MODELS: 1998 CHEVROLET AND GMC TRUCK P32/42 MODELS

THIS BULLETIN REVISES DIAGNOSTIC, "FUEL GAUGE INACCURATE" ON PAGE 8AB81-5, IN THE 1998 P32/42 SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 02

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.