Front Wheel Speed Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the front wheel speed sensor electrical connector (1).

Caution: Refer to Vehicle Lifting Caution in the Preface section.

3. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the wheel. Refer to Tire and Wheel Removal and Installation .
5. Remove the bolts (1) and the front wheel speed sensor (2) from the steering knuckle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front wheel speed sensor (2) to the steering knuckle. Secure it with the bolts (1).

Tighten
Tighten the front wheel speed sensor bolt to 23 N·m (17 lb ft).

2. Install the wheel. Refer to Tire and Wheel Removal and Installation .
3. Lower the vehicle.
4. Connect the front wheel speed sensor electrical connector (1).
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .