Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Mounting Bracket Bolts | 35-45 N·m | 25-33 lb ft
A/C Compressor Mounting Lower Bolts | 20-24 N·m | 15-18 lb ft
A/C Compressor Mounting Upper Bolts | 18-22 N·m | 13-16 lb ft
Air Filter Housing Nuts | 5-7 N·m | 44-62 lb in
Air Filter Snorkel Bolt | 7-9 N·m | 62-80 lb in
Camshaft Gear Bolt | 50-60 N·m | 36-44 lb ft
Camshaft Plate Screw | 9-12 N·m | 80-106 lb in
Clutch Housing Lower Plate Bolts | 4-7 N·m | 35-62 lb in
Connecting Rod Bearing Cap Nuts | 31-35 N·m | 23-25 lb ft
Crankshaft Pulley Bolt | 65-75 N·m | 48-55 lb ft
Crankshaft Main Bearing Cap Bolts | 55-60 N·m | 41-44 lb ft
Crankshaft Rear Oil Seal Housing Bolts/Screws | 9-12 N·m | 80-106 lb in
Cylinder Head Bolts | 85-90 N·m | 63-66 lb ft
Cylinder Head Cover Hexagon Bolts | 9-12 N·m | 80-106 lb in
Distributor Housing Bolts/Nuts | 9-12 N·m | 80-106 lb in
Engine Mount Brace Bracket Bolts | 35-45 N·m | 25-33 lb ft
Engine Mount Brace Bracket Nuts | 18-22 N·m | 13-16 lb ft
Engine Mount Damping Block Bolts | 45-55 N·m | 33-41 lb ft
Engine Mount Front Bracket-to-Engine Mount Bolt | 35-41 N·m | 25-30 lb ft
Engine Mount Front Damping Bush Bolt--Crossmember Side | 35-41 N·m | 25-30 lb ft
Engine Mount Front Damping Bush Bolts--Crossmember Side | 45-55 N·m | 33-41 lb ft
Engine Mount Front Damping Bush Bolt/Nut--Bracket Side | 68-83 N·m | 50-62 lb ft
Engine Mount Intermediate Bracket Bolts | 72-88 N·m | 53-65 lb ft
Engine Mount Intermediate Bracket Upper Nuts | 60-70 N·m | 44-52 lb ft
Engine Mount Lower Bracket Bolts | 35-41 N·m | 25-30 lb ft
Engine Mount Reaction Rod-to-Body Bolts | 68-83 N·m | 50-61 lb ft
Engine Mount Reaction Rod-to-Engine Mount Bolts/Nuts | 68-83 N·m | 50-61 lb ft
Engine Mount Upper Bracket Bolts | 35-41 N·m | 25-30 lb ft
Exhaust Manifold Bolts/Nuts | 17-27 N·m | 13-20 lb ft
Exhaust Manifold Heat Shield Bolts | 8-12 N·m | 71-106 lb in
Flywheel Bolts | 40-45 N·m | 30-33 lb ft
Intake Manifold Main Bracket Bolt (12 M) | 18-22 N·m | 13-16 lb ft
Intake Manifold Main Bracket Bolts (10 M) | 9-12 N·m | 80-106 lb in
Intake Manifold Main Bracket Nuts | 9-12 N·m | 80-106 lb in
Intake Manifold Nuts | 15-19 N·m | 11-14 lb ft
Intake Manifold Subsidiary Bracket Bolt | 18-22 N·m | 13-16 lb ft
Intake Manifold Subsidiary Bracket Nut | 15-19 N·m | 11-14 lb ft
Oil Filter | 12-16 N·m | 106-140 lb in
Oil Filter Stud | 20-25 N·m | 15-18 lb ft
Oil Level Gage Guide Tube Bolt | 9-12 N·m | 80-106 lb in
Oil Pan Bolts/Nuts | 9-12 N·m | 80-106 lb in
Oil Pan Drain Plug | 30-40 N·m | 22-30 lb ft
Oil Pressure Switch | 12-16 N·m | 106-140 lb in
Oil Pump Cover Bolts | 9-12 N·m | 80-106 lb in
Oil Pump Strainer Bolt | 9-12 N·m | 80-106 lb in
Power Steering Pump Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Front Bracket Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Rear Bracket Adjust Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Rear Bracket Bolt | 18-22 N·m | 13-16 lb ft
Power Steering Pump Rear Bracket Nut | 20-24 N·m | 15-18 lb ft
Rocker Arm Shaft Bolts | 9-12 N·m | 80-106 lb in
Spark Plug | 20-30 N·m | 15-22 lb ft
Timing Belt Front Lower Cover Bolts | 9-12 N·m | 80-106 lb in
Timing Belt Front Upper Cover Bolts | 9-12 N·m | 80-106 lb in
Timing Belt Rear Cover Bolts | 9-12 N·m | 80-106 lb in
Timing Belt Tensioner Bolt | 15-23 N·m | 11-17 lb ft
Valve Adjusting Lock Nuts | 15-20 N·m | 11-15 lb ft