Power Windows Inoperative - All. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Window Systems Connector End Views Connector End View Reference: Moveable Window Schematics
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Verify that the all power windows inoperative fault is present. Do the power windows operate normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3

3

1. Disconnect the driver window switch.
2. Turn ON the ignition, with the engine OFF.
3. Probe the 30 A power fuse voltage circuit of the driver window switch with a test lamp that is connected to a good ground.

Does the test lamp illuminate?

Go to Step 4

Go to Step 5

4 | Connect a test lamp between the 30A power fuse voltage circuit of the driver window switch and the ground circuit of the driver window switch. Does the test lamp illuminate? | Go to Step 6 | Go to Step 7
5 | Test the 30A power fuse voltage circuit of the driver window switch for a short to ground or an open. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 9 | --
6 | Inspect for poor connections at the harness connector of the driver window switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 9 | Go to Step 8
7 | Repair the open in the ground circuit. Refer to Wiring Repairs . Did you complete the repair? | Go to Step 9 | --
8 | Replace the driver window switch. Did you complete the replacement? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2