Front Side Door Window Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front door seal trim. Refer to Door Water Deflector Replacement .
2. Remove the outside rearview mirror from the front door. Refer to Outside Rearview Mirror Replacement .
3. Remove the division bar screw.
4. Remove the inside bolt (4).
5. Remove the outside bolt (3).
6. Remove the division bar (2).
7. Remove the glass run from the front door.

Notice: When removing glass from the vehicle, apply tape to corners of glass and adjacent surfaces to help prevent paint damage.

8. Remove the glass retaining bolts (2).
9. Remove the glass from the front door (1).

### Installation Procedure

1. Install the front door glass with the bolts.
2. Install the front door glass run.
3. Install the division bar with the guide rail inside bolt, the guide rail outside bolt and the guide rail screw.
4. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
5. Install the front door seal trim. Refer to Door Water Deflector Replacement .