Door Check Link Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement .
2. Remove the door check link-to-body bolt (2).
3. Remove the door check link-to-door bolts (3).
4. Remove the door check link (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the door check link (1) to the door and the body with the bolts (2, 3).

Tighen

• | Tighten the door check link to body bolt to 35 N·m (26 ft lb).

• | Tighten the door check link to door bolt to 5 N·m (44 in lb).

2. Remove the door seal trim. Refer to Door Water Deflector Replacement .