Horn Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the electrical connector.
3. Remove the power steering reservoir tank.
4. Remove the nut and the horn.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the horn with the nut.

Tighten
Tighten the horn nut to 20 N·m (15 lb ft).

2. Install the power steering reservoir tank.
3. Connect the electrical connector.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.