High Mount Stop Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the liftgate.
3. Remove the center high-mounted stop lamp (CHMSL) cover and screws.
4. Remove the CHMSL screws.
5. Remove the CHMSL.
6. Remove the bulb.

### Installation Procedure

1. Install the CHMSL bulb.
2. Install the CHMSL with the screws.
3. Install the CHMSL cover with the screws.
4. Connect the negative battery cable.
5. Close the liftgate.