Brake Fluid Level Indicator Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the vacuum hose from the power booster. Refer to Vacuum Brake Booster Check Valve and/or Hose Replacement .
2. Remove the brake fluid level switch locking system by the flathead screwdriver (1).
3. Remove the brake fluid level switch.
4. Disconnect the electrical connector (1).

### Installation Procedure

1. Install the brake fluid level switch.
2. Connect the electrical connector.
3. Install the vacuum hose to the power booster. Refer to Vacuum Brake Booster Check Valve and/or Hose Replacement .