Air Cleaner Assembly Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the air filter housing.
2. Disconnect the intake tube clamp (2).
3. Disconnect the air intake tube from the air filter housing (1).
4. Remove the snorkel bolt (1).
5. Remove the air filter housing bolts (2).
6. Remove the air filter housing (3), resonator, and snorkel assembly from the bracket (4).
7. Remove the snorkel from the resonator pressing the part of hook (1).
8. Remove the resonator (2) from the air filter housing pressing the art of hook (4).

### Installation Procedure

1. Install the resonator to the air filter housing (2).
2. Install the snorkel the resonator (1).
3. Install the snorkel assembly, resonator, and air filter housing (3) onto bracket (4).

Notice: Refer to Fastener Notice in the Preface section.

4. Install air filter housing bolts (2).

Tighten
Tighten the bolts to: 7-9 N·m (62-80 lb-in)

5. Install the snorkel bolt (1).
6. Connect the air intake tube to the air filter housing (1).
7. Connect the electrical connector on the air filter housing.