Diagnostic Trouble Code (DTC) List - Vehicle. Chevrolet Joy 2008

For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
15 |  | TCM | DTC 15
17 |  | TCM | DTC 17
22 |  | TCM | DTC 22
41 |  | TCM | DTC 41
43 |  | TCM | DTC 43
44 |  | TCM | DTC 44
48 |  | TCM | DTC 48
53 |  | TCM | DTC 53
54 |  | TCM | DTC 54
55 |  | TCM | DTC 55
58 |  | TCM | DTC 58
75 |  | TCM | DTC 75
B0016 | Passenger Frontal Deployment Loop Resistance Low | SDM | DTC B0016, B0017, or B0018
B0017 | Passenger Frontal Deployment Loop Open | SDM | DTC B0016, B0017, or B0018
B0018 | Passenger Frontal Deployment Loop Out of Range | SDM | DTC B0016, B0017, or B0018
B0022 | Driver Frontal Deployment Loop Resistance Low | SDM | DTC B0022, B0024, or B0026
B0024 | Driver Frontal Deployment Loop Out of Range | SDM | DTC B0022, B0024, or B0026
B0026 | Driver Frontal Deployment Loop Open | SDM | DTC B0022, B0024, or B0026
B0028 | RF Side Deployment Loop Resistance Low | SDM | DTC B0028, B0029, or B0030
B0029 | RF Side Deployment Loop Open Circuit | SDM | DTC B0028, B0029, or B0030
B0030 | RF Side Deployment Loop Voltage Out of Range | SDM | DTC B0028, B0029, or B0030
B0040 | LF Side Deployment Loop Resistance Low | SDM | DTC B0040, B0041, or B0045
B0041 | LF Side Deployment Loop Open Circuit | SDM | DTC B0040, B0041, or B0045
B0045 | LF Side Deployment Loop Voltage Out of Range | SDM | DTC B0040, B0041, or B0045
B0051 | Deployment Commanded | SDM | DTC B0051
B0053 | Deployment Commanded With Loop Faults Present | SDM | DTC B0053
B0057 | RF Pretensioner Deployment Loop Resistance Low | SDM | DTC B0057
B0058 | RF Pretensioner Deployment Loop Open | SDM | DTC B0058
B0059 | RF Pretensioner Deployment Loop Voltage Out of Range | SDM | DTC B0059
B0061 | Warning Lamp Circuit Open or Short to Ground | SDM | DTC B0061
B0064 | LF Pretensioner Deployment Loop Resistance Low | SDM | DTC B0064, B0065, or B0066
B0065 | LF Pretensioner Deployment Loop Open | SDM | DTC B0064, B0065, or B0066
B0066 | LF Pretensioner Deployment Loop Voltage Out of Range | SDM | DTC B0064, B0065, or B0066
B0077 | Left SIS Malfunction | SDM | DTC B0077
B0078 | Right SIS Malfunction | SDM | DTC B0078
B0079 | Incorrect Left SIS Installed | SDM | DTC B0079
B0080 | Discard Left SIS | SDM | DTC B0080
B0081 | Incorrect Right SIS Installed | SDM | DTC B0081
B0082 | Discard Right SIS | SDM | DTC B0082
B1000 | ECU Malfunction | SDM | DTC B1000
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035
C0036 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C0036
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0040
C0041 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C0041
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0045
C0046 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C0046
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0050
C0051 | Right Rear Wheel Speed Circuit Range Performance | EBCM | DTC C0051
C0060/C0065 | Left Front Dump Solenoid Circuit Open | EBCM | DTC C0060/C0065
C0070/C0075 | Right Front Dump Solenoid Circuit Open | EBCM | DTC C0070/C0075
C0080/C0085 | Left Rear Dump Solenoid Circuit Open | EBCM | DTC C0080/C0085
C0090/C0095 | Right Rear Dump Solenoid Circuit Open | EBCM | DTC C0090/C0095
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0121 | ABS Relay Circuit | EBCM | DTC C0121
C0161 | Stop Lamp Switch Circuit Open | EBCM | DTC C0161
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0800 | Battery Voltage Out of Range | EBCM | DTC C0800
C1395 | Fill and Bleed Not Complete | EBCM | DTC C1395
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030 or P0036 for the 0.8L engine or DTC P0030 or P0036 for the 1.0L engine
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030 or P0036 for the 0.8L engine or DTC P0030 or P0036 for the 1.0L engine
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0107 or P0108 for the 0.8L engine or DTC P0107 or P0108 for the 1.0L engine
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0107 or P0108 for the 0.8L engine or DTC P0107 or P0108 for the 1.0L engine
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112 or P0113 for the 0.8L engine or DTC P0112 or P0113 for the 1.0L engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112 or P0113 for the 0.8L engine or DTC P0112 or P0113 for the 1.0L engine
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118 for the 0.8L engine or DTC P0117 or P0118 for the 1.0L engine
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118 for the 0.8L engine or DTC P0117 or P0118 for the 1.0L engine
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM | DTC P0122 or P0123 for the 0.8L engine or DTC P0122, P0123, P0222, or P0223 for the 1.0L engine
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM | DTC P0122 or P0123 for the 0.8L engine or DTC P0122, P0123, P0222, or P0223 for the 1.0L engine
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0137 for the 0.8L engine or DTC P0131 or P0137 for the 1.0L engine
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0138 for the 0.8L engine or DTC P0132 or P0138 for the 1.0L engine
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 for the 0.8L engine or DTC P0133 for the 1.0L engine
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0131 or P0137 for the 0.8L engine or DTC P0131 or P0137 for the 1.0L engine
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0132 or P0138 for the 0.8L engine or DTC P0132 or P0138 for the 1.0L engine
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0140 for the 0.8L engine or DTC P0140 for the 1.0L engine
P0171 | Fuel Trim System Lean | ECM | DTC P0171 or P0172 for the 0.8L engine or DTC P0171 or P0172 for the 1.0L engine
P0172 | Fuel Trim System Rich | ECM | DTC P0171 or P0172 for the 0.8L engine or DTC P0171 or P0172 for the 1.0L engine
P0222 | Idle Speed Control (ISC) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.0L engine
P0223 | Idle Speed Control (ISC) Motor Position Sensor Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.0L engine
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, or P0268 for the 0.8L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.0L engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0300 | Engine Misfire Detected | ECM | DTC P0300 for the 0.8L engine or DTC P0300 for the 1.0L engine
P0327 | Knock Sensor (KS) Circuit Low Frequency | ECM | DTC P0327 for the 0.8L engine or DTC P0327 for the 1.0L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335, P0336, or P0337 for the 0.8L engine or DTC P0335, P0336, or P0337 for the 1.0L engine
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0337 for the 0.8L engine or DTC P0335, P0336, or P0337 for the 1.0L engine
P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM | DTC P0335, P0336, or P0337 for the 0.8L engine or DTC P0335, P0336, or P0337 for the 1.0L engine
P0341 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 or P0342 for the 0.8L engine or DTC P0341 or P0342 for the 1.0L engine
P0342 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0341 or P0342 for the 0.8L engine or DTC P0341 or P0342 for the 1.0L engine
P0351 | Ignition Coil 1 Control Circuit | ECM | DTC P0351, P0352, or P0353 for the 0.8L engine or DTC P0351 or P0352 for the 1.0L engine
P0352 | Ignition Coil 2 Control Circuit | ECM | DTC P0351, P0352, or P0353 for the 0.8L engine or DTC P0351 or P0352 for the 1.0L engine
P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351, P0352, or P0353
P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM | DTC P0400, P0401, P0402, or P1402 for the 0.8L engine or DTC P0400, P0401, P0402, or P1402 for the 1.0L engine
P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM | DTC P0400, P0401, P0402, or P1402 for the 0.8L engine or DTC P0400, P0401, P0402, or P1402 for the 1.0L engine
P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 0.8L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.0L engine
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 0.8L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.0L engine
P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 0.8L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.0L engine
P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 0.8L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.0L engine
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 for the 0.8L engine or DTC P0420 for the 1.0L engine
P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0444 or P0445 for the 0.8L engine or DTC P0444 or P0445 for the 1.0L engine
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445 for the 0.8L engine or DTC P0444 or P0445 for the 1.0L engine
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0480 | Cooling Fan Relay Control Circuit 1 | ECM | DTC P0480 or P0481
P0481 | Coolant Fan Relay 2 and 3 Control Circuit | ECM | DTC P0480 or P0481
P0501 | Vehicle Speed Sensor (VSS) Performance | ECM | DTC P0501 for the 0.8L engine or DTC P0501 for the 1.0L engine
P0510 | Idle Speed Control (ISC) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0510
P0511 | Idle Air Control (IAC) System | ECM | DTC P0511
P0537 | Air Conditioning (A/C) Evaporator Temperature Sensor Circuit Low Voltage | ECM | DTC P0537
P0538 | Air Conditioning (A/C) Evaporator Temperature Sensor Circuit High Voltage | ECM | DTC P0538
P0562 | System Voltage Too Low | ECM | DTC P0562
P0563 | System Voltage Too High | ECM | DTC P0563
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 0.8L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.0L engine
P0604 | Control Module Random Accessory Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 0.8L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.0L engine
P0605 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 0.8L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.0L engine
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629 for the 0.8L engine or DTC P0628 or P0629 for the 1.0L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629 for the 0.8L engine or DTC P0628 or P0629 for the 1.0L engine
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0646 or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0646 or P0647
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P0650 or P1650 for the 0.8L engine or DTC P0650 or P1650 for the 1.0L engine
P0654 | Engine Speed Output Circuit | ECM | DTC P0654
P0656 | Fuel Level Output Circuit | ECM | DTC P0656
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 0.8L engine or DTC P0700 for the 1.0L engine
P0705 | Transmission Range (TR) Switch Circuit | ECM | DTC P0705
P0710 |  | ECM | DTC P0710
P0715 |  | ECM | DTC P0715
P0720 | Vehicle Speed Sensor Circuit | ECM | DTC P0720
P0740 | Torque Converter Clutch (TCC) Electrical Circuit | ECM | DTC P0740
P0741 | Torque Converter Clutch (TCC) Stuck Off | ECM | DTC P0741
P0748 | Pressure Control Solenoid Control Circuit | ECM | DTC P0748
P0753 | Shift Solenoid A | ECM | DTC P0753
P0758 | Shift Solenoid B | ECM | DTC P0758
P1390 | Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396 for the 0.8L engine or DTC P1390 or P1396 for the 1.0L engine
P1396 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1390 or P1396 for the 0.8L engine or DTC P1390 or P1396 for the 1.0L engine
P1402 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM | DTC P0400, P0401, P0402, or P1402 for the 0.8L engine or DTC P0400, P0401, P0402, or P1402 for the 1.0L engine
P1504 | Transmission Control Module (TCM) Communication Performance | ECM | DTC P1504 for the 0.8L engine or DTC P1504 for the 1.0L engine
P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611 for the 0.8L engine or DTC P1610 or P1611 for the 1.0L engine
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611 for the 0.8L engine or DTC P1610 or P1611 for the 1.0L engine
P1628 | Theft Deterrent Start Enable Signal Not Received | ECM | DTC P1628
P1629 | Theft Deterrent Start Enable Signal Not Correct | ECM | DTC P1629
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P0650 or P1650 for the 0.8L engine or DTC P0650 or P1650 for the 1.0L engine
P1668 | Engine Coolant Temperature (ECT) Output Circuit | ECM | DTC P1668
P1795 | Pressure Control Solenoid Ground Return Circuit Malfunction | ECM | DTC P1795
P2101 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P2101, P2118, or P2119
P2118 | Idle Speed Control (ISC) System | ECM | DTC P2101, P2118, or P2119
P2119 | Idle Speed Control (ISC) System Performance | ECM | DTC P2101, P2118, or P2119