Low and High Beams Headlamps Inoperative. Chevrolet Joy 2008

For 1990-2009 cars

### Diagnostic Aids

If there are several other symptoms, including an inoperative radiator fan, the windshield washer pump, or the turn signal lamps, check ground G102 and G104.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Check fuses Ef24, Ef18, Ef17, and F14. Are any fuses blown? | -- | Go to Step 2 | Go to Step 4

2

1. Check for a short circuit and repair it, if necessary.
2. Replace the fuse.

Is the repair complete?

--

Go to Step 3

--

3 | Turn the low beam headlamps on. Do the low beam headlamps work? | -- | Go to Step 6 | Go to Step 4
4 | Check the low beam headlamps system. Refer to Headlamps Inoperative - Low Beams . Is any problem found? | -- | Go to Step 5 | --
5 | Repair the problem. Is the repair complete? | -- | Go to Step 6 | --
6 | Turn the high beam headlamps on. Do the high beam headlamps work? | -- | System OK | Go to Step 7
7 | Check the high beam headlamps system. Refer to Headlamps Inoperative - High Beams . Is any problem found? | -- | Go to Step 8 | --
8 | Repair the problem. Is the repair complete? | -- | System OK | --