Manifold Absolute Pressure Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the manifold absolute pressure (MAP) sensor connector.
2. Remove the MAP sensor bolts and the MAP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the MAP sensor with the bolts.

Tighten
Tighten the MAP sensor bolts/nuts to 8-12 N·m (71-106 lb in).

2. Connect the MAP sensor connector.