Air Cleaner Assembly Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the intake tube clamp (2).
2. Disconnect the electrical connector from the air filter housing.
3. Disconnect the air intake tube from the air filter housing (1).
4. Remove the snorkel bolt (1).
5. Remove the air filter housing bolts (2).
6. Remove the air filter housing, resonator, and snorkel assembly (3) from the bracket (4).

Important: Remove the air filter, resonator, and snorkel assembly separately.

7. Remove the snorkel from the resonator pressing the part of hook (3).
8. Remove the resonator (2) from the air filter housing pressing the part of hook (4).

### Installation Procedure

1. Install the resonator on to the air filter housing.
2. Install the snorkel on to the resonator.
3. Install the air filter housing, resonator, and snorkel assembly to the bracket.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the air filter housing and snorkel bolts.

Tighten
Tighten the fuel tank strap bolts to 7-9 N·m (62-80 lb in).

5. Connect the air intake tube on the air filter housing (1).
6. Connect electrical connector to the air filter housing.
7. Connect the intake tube clamp (2).