Release Bearing Replacement. Chevrolet Joy 2008

For 1990-2009 cars

## Release Bearing Replacement Y4M

#### Tools Required

• | DT 47513 (DW 210-030) Bushing Joint Pipe

• | DT 47514 (DW 210-040) Bushing Remover/Installer

• | J 2619-01 (09930-30102) Slide Hammer

• | 09943-88211 Bushing, Bearing Installer

• | 09923 46040 Bushing Joint Pipe

### Removal Procedure

1. Remove the transaxle from the vehicle. Refer to Transmission Replacement for the Y4M transmission.
2. Remove the release arm. Refer to Clutch Release Arm Replacement .
3. Remove the release bearing.
4. Remove the No. 2 bushing and seal using DT 47514 (2) and a hammer.
5. Remove the release shaft (1).
6. Insert the tap (M14X1.5) to the No. 1 bushing (1).
7. Insert DT 47514 (1) into the tab.
8. Connect J 2619-01 (2) to the end of DT 47513 .
9. Remove the No. 1 bushing by pulling.

### Installation Procedure

1. Install the No. 1 release shaft bushing using 09923 46040 (1) , DT 47513 (2), and a hammer.
2. Install the No. 2 release shaft bushing and seal using DT 47514 (1) and a hammer.
3. Coat the spline of the transaxle input shaft with multi-purpose grease (1).
4. Coat the release bearing bore and the connecting of the release shaft with multi-purpose grease (2).
5. Install the release bearing.
6. Install the release arm. Refer to Clutch Release Arm Replacement .
7. Install the transaxle to the vehicle. Refer to Transmission Replacement for the Y4M transmission.