Front Fog Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front wheels. Refer to Tire and Wheel Removal and Installation .
3. Remove the wheelhouse splash shield (1). Refer to Fender Liner Replacement .
4. Remove the front fog lamp screws (1).
5. Disconnect the electrical connector (2).
6. Remove the front fog lamp (3).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front fog lamp (3) with the screws (1).

Tighten
Tighten the screws to 4 N·m (35 lb in).

2. Connect the front fog lamp connector (2).
3. Install the front wheelhouse splash shield. Refer to Fender Liner Replacement .
4. Install the front wheels. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.
6. Connect the negative battery cable.