Coolant Pump Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the lower radiator hose and drain the coolant. Refer to Cooling System Draining and Filling .
3. Remove the rear timing belt cover bolts (1).
4. Remove the rear timing belt cover (2).
5. Remove the coolant pump nuts (2).
6. Remove the bolts (1).
7. Remove the coolant pump (3, 4).
8. Remove the gasket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the coolant pump with the new gasket.
2. Install the coolant pump bolts (1).

Tighten
Tighten the bolts and the nuts to 9-12 N·m (80-106 lb in).

3. Install the rear timing belt cover and bolts (1).

Tighten
Tighten the bolts to 9-12 N·m (80-106 lb in).

4. Install the timing belt. Refer to Timing Belt Replacement for the 0.8L engine or Timing Belt Replacement for the 1.0L engine.
5. Connect the lower radiator hose and fill the coolant. Refer to Cooling System Draining and Filling .
6. Connect the negative battery cable.