Power Steering Pump Belt Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front passenger side headlamp. Refer to Headlamp Replacement .
2. Loosen the rear bracket adjusting bolt (1).
3. Loosen the bolt (2).
4. Loosen the front bracket adjusting bolts (2).
5. Push the pump forward (1) and remove the drive belt pump.

### Installation Procedure

1. Install the pump drive belt.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front bracket adjusting bolt (1).

Tighten
Tighten the front bracket adjusting bolt to 18-22 N·m (13-16 lb ft).

3. Install the rear bracket adjusting bolt (3).

Tighten
Tighten the rear bracket adjusting bolt to 20-24 N·m (15-18 lb ft).

4. Install the drive belt pump (2).

Tighten
Tighten the power steering pump bolt to 20-24 N·m (15-18 lb ft).

5. Install the front passenger side headlamp. Refer to Headlamp Replacement .