Brake Pad Inspection. Chevrolet Joy 2008

For 1990-2009 cars

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .

Caution: Refer to Brake Dust Caution in the Preface section.

Notice: Refer to Brake Caliper Notice in the Preface section.

2. Remove the front wheels. Refer to Tire and Wheel Removal and Installation .
3. Visually inspect the linings for minimum thickness and wear.
4. Measure the thickness.

Specification
The minimum thickness of the pad friction material and the backing plate is 8 mm (0.31 in).

5. If the thickness of the pads are less than the specification, replace the pads. Install the shoe and linings in axle sets only. Refer to Front Disc Brake Pads Replacement .
6. Install the front wheels. Refer to Tire and Wheel Removal and Installation .
7. Lower the vehicle.