Liftgate Lock Cylinder Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the tailgate.
3. Remove the rear window wiper motor assembly. Refer to Rear Window Wiper Motor Replacement .
4. Disconnect the tailgate lock rod (3).
5. Remove the nuts from the tailgate lock cylinder (2).
6. Remove the tailgate lock cylinder (1).

### Installation Procedure

1. Install the tailgate lock cylinder (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the tailgate lock cylinder (2).

Tighten
Tighten the tailgate lock cylinder nuts (2) to 5 N·m (44 in lb).

3. Connect the tailgate lock rod (3).
4. Install the rear window wiper motor assembly. Refer to Rear Window Wiper Motor Replacement .
5. Connect the negative battery cable.