Liftgate Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear cargo area trim panel. Refer to Cargo Area Rear Trim Panel Replacement.
3. Disconnect the tailgate electrical connector.
4. Remove the tailgate strut. Refer to Liftgate Window Strut Replacement .
5. Remove the hinge bolts.
6. Disconnect the body-to-tailgate rubber grommet.
7. Remove the tailgate.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the body-to-tailgate rubber grommet.
2. With the aid of another technician, lightly secure the tailgate with the bolts.
3. Adjust the tailgate for proper fit.
4. Install the tailgate strut. Refer to Liftgate Window Strut Replacement .
5. Connect the tailgate electrical connector.
6. Install the rear cargo area trim panel. Refer to Cargo Area Rear Trim Panel Replacement.
7. Connect the negative battery cable.