Fluid and Lubricant Recommendations. Chevrolet Joy 2008

For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO JWS 3314
Brake Fluid | DOT-3 or DOT-4
Clutch Linkage Pivot Points | Grease
Engine Coolant | Phosphate Based Coolant

Engine Oil

• | API SM ILSAC GF-IV Grade SAE 10W-30

• | Cold area: SAE 5W-30

• | Hot area: SAE 15W-40/10W-30

Hood Latch Assembly | Grease
Hood and Door Hinges, Fuel Door Hinge, Rear Compartment Lid Hinges | Spray type grease
Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W-85
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® II-D
Parking Brake Cable | Grease
Weatherstrips | Silicone Grease