Fuel Tank Filler Door Latch Release Cable Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front door sill plate. Refer to Front Side Door Sill Plate Replacement .
2. Remove the fuel filler door remote handle screws (3).
3. Disconnect the cable (1).
4. Remove the fuel filler door remote handle (2).
5. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
6. Remove the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .
7. Remove the cargo area rear trim panel. Refer to Cargo Area Rear Trim Panel Replacement .
8. Remove the lock striker (1) of the fuel filter by turning it rectangularly.
9. Remove the fuel filler door remote cable retaining strip.
10. Disconnect the fuel filler door remote cable (1).

### Installation Procedure

1. Connect the fuel filler door remote cable (1) to the fuel filler door.
2. Retain the cable with the strip.
3. Install the lock striker of the fuel filler.
4. Install the cargo area rear trim panel. Refer to Cargo Area Rear Trim Panel Replacement .
5. Install the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .
6. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
7. Connect the fuel filler door remote cable to the handle.
8. Install the fuel filler door remote handle with the screws.
9. Install the front door sill plate. Refer to Front Side Door Sill Plate Replacement .