Instrument Panel Outer Trim Cover Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.

Notice: The instrument panel (I/P) should be at room temperature before performing service. This will allow the I/P to be more pliable. To prevent the instrument panel damage, cover the flat bladed tool with a soft cloth.

2. Remove the instrument cluster trim panel from the instrument panel.
3. Disconnect the hazzard lamp switch connector.

### Installation Procedure

1. Connect the hazzard lamp switch electrical connector.
2. Install the instrument cluster trim panel.
3. Connect the negative battery cable.