Rear Door Opening Frame Garnish Molding Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Pry off the interior garnish molding. Refer to Rear Door Upper Garnish Molding Replacement .
2. Remove the exterior garnish molding screw (1).
3. Pry off the exterior garnish molding (2).

### Installation Procedure

1. Install the exterior garnish molding with the screw.
2. Install the interior garnish molding. Refer to Rear Door Upper Garnish Molding Replacement .