Ignition System Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Firing Order | 1-3-2
Spark Plug Wire Resistance | 1,800-8,000 Ohms
Spark Plug Gap - Leaded | 0.8 mm | 0.031 in
Spark Plug Gap - Unleaded | Bosch - 1.1 mm, NGK - 1.2 mm | Bosch - 0.043 in, NGK - 0.047 in
Spark Plug Torque | 25 N·m | 18 lb ft
Spark Plug Type - Leaded | Bosch - WR8DC, NGK - BPR5EY
Spark Plug Type - Unleaded | Bosch - WR8DCX, NGK - BPR5EY-11