Fuel Gage Inaccurate or Inoperative. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Instrument Cluster Schematics

1

1. Connect a scan tool.
2. Check for engine control diagnostic trouble codes (DTCs).

Is the vehicle speed sensor DTC set?

--

Go to Diagnostic Trouble Code (DTC) List - Vehicle

Go to Step 2

2

1. Turn the ignition OFF.
2. Disconnect the engine control module (ECM) connector.
3. Remove the instrument cluster.
4. Check continuity between the ECM terminal 64 for the 0.8 L engine or terminal 40 for the 1.0 L engine and the instrument panel cluster (IPC) connector terminal 13.

Does the ohmmeter indicate the specified value?

0ohms

Go to Step 4

Go to Step 3

3 | Repair the open circuit between the ECM terminal 64 for the 0.8 L engine or terminal 40 for the 1.0 L engine and the instrument panel cluster (IPC) connector terminal 13. Is the repair complete? | -- | System OK | --
4 | Replace the fuel gauge. Is the repair complete? | -- | Go to Diagnostic System Check - Vehicle | --