Exhaust Muffler Replacement. Chevrolet Joy 2008

For 1990-2009 cars

## Exhaust Muffler Replacement Front

### Removal Procedure

Caution: Refer to Hot Exhaust System Caution in the Preface section.

1. Remove the front exhaust pipe-to-front muffler nuts (1).
2. Remove the front muffler-to-rear muffler nuts.
3. Detach the front muffler from rubber hanger and remove the front muffler.

### Installation Procedure

1. Hang the front muffler to rubber hanger.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front muffler-to-rear muffler nuts.

Tighten
Tighten the nuts to 25 - 35 N·m (18 - 25 lb ft).

3. Install the exhaust pipe-to-front muffler nuts (1).

Tighten
Tighten the nuts to 25 - 35 N·m (18 - 25 lb ft).

## Exhaust Muffler Replacement Rear

### Removal Procedure

1. Remove the front muffler-to rear muffler nuts.
2. Detach the rear muffler from the rubber hangers.
3. Remove the rear muffler.

### Installation Procedure

1. Install rear muffler.
2. Attach rear muffler to rubber hangers.

Notice: Refer to Fastener Notice in the Preface section.

3. Install front muffler to rear muffler nuts.

Tighten
Tighten the nuts to 25 - 35 N·m (18 - 25 lb ft).