Power Steering Fluid Reservoir Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the fluid reservoir by pulling it upward (1).
2. Disconnect the supply line hose by loosening the hose clamp (3).
3. Remove the reservoir cap (1).
4. Catch the escaping fluid in a drain pan.
5. Disconnect the fluid return hose by loosening the hose clamp (2).
6. Plug the openings of both hoses to prevent the fluid loss and contamination.

### Installation Procedure

1. Connect both hoses and secure the hose clamps.
2. Fill the fluid reservoir with power steering fluid.
3. Inspect for leaks. If there are leaks, correct the cause of the leaks and bleed the system. Refer to Power Steering System Bleeding .