Quarter Lower Rear Trim Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the tailgate.
3. Remove the seat back.
4. Remove the rear seat parcel shelf. Refer to Rear Window Shelf Trim Panel Replacement .
5. Remove the rear speaker from the rear parcel shelf. Refer to Radio Rear Speaker Replacement .
6. Remove the rear parcel side shelf screws (2).
7. Remove the rear parcel side shelf (1).

### Installation Procedure

1. Install the rear parcel side shelf with the screw.
2. Install the rear speaker to the rear parcel shelf. Refer to Radio Rear Speaker Replacement .
3. Install the rear parcel shelf. Refer to Rear Window Shelf Trim Panel Replacement .
4. Install the seat back.
5. Connect the negative battery cable.