Quarter Upper Trim Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the tailgate.
3. Disconnect the rear speaker electrical connector.
4. Remove the rear parcel side shelf. Refer to Rear Window Shelf Trim Panel Replacement .
5. Remove the rear seat back.
6. Remove the rear seat belt bolt on the rear quarter upper trim panel. Refer to Rear Seat Back Replacement .
7. Pry off the rear quarter upper trim panel (1).

### Installation Procedure

1. Install the rear quarter upper trim panel.
2. Install the rear seat belt bolt on the rear quarter upper trim panel. Refer to Rear Seat Back Replacement .
3. Install the rear seat back.
4. Install the rear parcel side shelf. Refer to Rear Window Shelf Trim Panel Replacement .
5. Connect the rear speaker connector.
6. Connect the negative battery cable.