Hood Primary and Secondary Latch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the hood latch screws (3).
3. Disconnect the hood latch release cable (2).
4. Remove the hood latch (1).

### Installation Procedure

1. Connect the hood latch release cable (2) to the latch (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hood latch (1) with the screws (3).

Tighten
Tighten the hood latch screws to 8.5 N·m (75 lb in).

3. Close the hood.