Generator Usage. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brushes Length - A-Type

- Standard

18.5 mm

0.728 in

- Limit

13.5 mm

0.531 in

Brushes Length - B-Type |  |

- Standard

20 mm

0.787 in

- Limit

14 mm

0.551 in

Output - Capacity

- A-Type

12 V, 65 A

- B-Type

12 V, 65 A

Regulator Voltage

- A-Type

14.4-15 V

- B-Type

14.3-4.9 V

Type

- A-Type

J114D (MANDO)

- B-Type

CS114D (DAC)