Hood Primary Latch Release Cable Handle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the hood latch nut (1) into the instrument panel.
2. Disconnect the hood latch release lever cable (1).
3. Remove the hood latch release lever (2).

### Installation Procedure

1. Connect the hood latch release cable to the hood latch lever.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hood latch lever release to the instrument panel with the hood latch nut.