Theft Deterrent Alarm Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the siren electrical connector.
4. Remove the siren bracket mounting bolt and siren.

### Installation Procedure

1. Install the siren with the mounting bolt.

Notice: Refer to Fastener Notice in the Preface section.

2. Connect the electrical connector.

Tighten
Tighten the siren mounting bolt to 8 N·m (71 lb in).

3. Lower the vehicle.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .