Rear Fog Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector.
3. Remove the screws.
4. Remove the rear fog lamp assembly from the vehicle.

### Installation Procedure

1. Install the rear fog lamp assembly with the screws.
2. Connect the electrical connector.
3. Connect the negative battery cable.