Rear Bumper Fascia Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the bolts (1) from underneath the fascia.
3. Remove the fascia plastic retainers from the rear bumper fascia.
4. Lower the vehicle.
5. Remove the nuts (1) in the luggage compartment.
6. Remove the screws (2).
7. Remove the fascia (3).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the fascia (3).
2. Install the fascia upper nut (1).

Tighten
Tighten the fascia upper nut to 4N·m (35 in lb).

3. Install the fascia upper screws (2).

Tighten
Tighten the upper fascia screws to 1.5 N·m (13 in lb).

Caution: Refer to Vehicle Lifting Caution in the Preface section.

4. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Install the rear fascia plastic clips.
6. Install the fascia lower bolts (1).
7. Lower the vehicle.