Rear Washer Always On. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Wiper/Washer Schematics Connector End View Reference: Wiper/Washer Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle

2

1. Disconnect the wiper/washer switch connector.
2. Turn the ignition switch ON, engine OFF.

Is the washer still ON?

Go to Step 3

Go to Step 4

3 | Repair the short to ground condition in the washer control circuit between the wiper/washer switch and the washer pump. Refer to Wiring Repairs . Is the repair complete? | Go to Step 5 | --
4 | Replace the wiper/washer switch. Is the replacement complete? | Go to Step 5 | --

5

1. Turn the ignition switch ON, engine OFF.
2. Operate the washer pump.

Does the washer pump operate properly?

System OK

--