Central Door Lock Actuator Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door seal trim. Refer to Door Water Deflector Replacement .
3. Remove the door lock assembly. Refer to Front Side Door Lock Replacement .
4. Remove the door lock assembly screws (1).
5. Remove the actuator from the door lock assembly (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the door lock actuator to the door lock assembly with the screws.

Tighten
Tighten the screws to 8 N·m (71 in lb).

2. Install the door lock assembly to the vehicle. Refer to Front Side Door Lock Replacement .
3. Install the door seal trim. Refer to Door Water Deflector Replacement .
4. Connect the negative battery cable.