Ignition Coil Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.

Important: Note the ignition wire location and disconnect the ignition wires from the electronic ignition (EI) system ignition coil.

2. Disconnect the EI system ignition coil connector.
3. Remove the EI system ignition coil retaining bolts.
4. Remove the EI system ignition coil.

### Installation Procedure

1. Install the EI system ignition coil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EI system ignition coil.

Tighten
Tighten the EI system ignition coil to 8-12 N·m (71-106 lb in).

3. Install the EI system ignition coil retaining bolts.
4. Connect the EI system ignition coil connector.
5. Connect the negative battery cable.