Door Window Regulator Replacement. Chevrolet Joy 2008

For 1990-2009 cars

## Door Window Regulator Replacement Manual

### Removal Procedure

1. Remove the glass. Refer to Front Side Door Window Replacement or Rear Side Door Window Replacement .
2. Remove the window regulator screws (1).
3. Remove the window regulator (2).

### Installation Procedure

1. Install the regulator with the screws.
2. Install the glass. Refer to Front Side Door Window Replacement or Rear Side Door Window Replacement .

## Door Window Regulator Replacement Power

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glass. Refer to Front Side Door Window Replacement or Rear Side Door Window Replacement .
3. Disconnect the window motor electrical connector (2).
4. Remove the screws (1).
5. Remove the window regulator assembly (3).
6. Remove the screws (1).
7. Remove the window regulator (2).
8. Remove the window motor from the window regulator.

### Installation Procedure

1. Install the window motor to the window regulator with the screws.
2. Install the window regulator assembly with the screws.
3. Connect the window motor electrical connector.
4. Install the glass. Refer to Front Side Door Window Replacement or Rear Side Door Window Replacement .
5. Connect the negative battery cable.